===========================================================================
                    Software Release Note
===========================================================================
Model Name : 
LGB1110A (GS-2610G)
LGB1126A-R2 (GS-2626G)
LGB5128A-R2 (FGS-2628KX)
Firmware Version : v6.54.2793 ~ v6.54.3160

[Changed]
==============================================================
* DMS: Web UI disable DMS and save start-config, the DMS is still enabled after reboot.

[Added]
==============================================================
* PM20190821001 - DMS: add Traffic Monitor features.

[Fixed]
==============================================================
*Bug 20028 - When switch is DHCP client, it will send DHCP discover with bootp flag unicast, if server reply unicast packet based on the flag, switch will can't IP from server.
*Bug 20074 - After applying ˇ§Don't show this message againˇ¨ in the Web UI, a prompt window will still pop up.
*Bug 20086 - DMS Diagnostics result is wrong when port is link down, it always shows "cable length is 0m".
*Bug 20118 - SNMP: Unable to set sysName OID=123.
*Bug 20200 - CLI: The message "poe device#1 not found / poe device#2 not found" is displayed at startup.
*Bug 20206 - SNMPv3 respones time is too long.
*Bug 20258 - CI: Send command ˇ§no snmp-server community v3 public/privateˇ¨ via Cli, the snmp-server community still displays the entry.